
   Magic Touch ProE-X & ProE Controller Installation for Win98, ME & 95 :

   1. If there is a previous installation of Magic Touch or other brand 
      touch screen driver on your computer, you must uninstall that driver first. 
   2. Insert the Magic Touch driver CD, the setup window appears.  
      (If the autorun is disabled on your computer, the setup window will not 
      open automatically, and you need to click the START button and RUN setup 
      from the CD.)
   3. Click to select the ProE controller.
   4. Click install button.
   5. When prompted for restarting the computer, plug in the ProE-X or ProE 
      controller and click OK.
   6. After the Windows is restarted, double click and open the Touch232 icon.  
      Click the calibration button to perform a 4-point calibration.
   7. Read user's manual for other functional options. 

Note: If installation wizard requests you to insert your 'Windows 98 cd,' you will need
to locate your Windows installation cd which should have come with your purchase of Windows
98.  Once located, point the wizard at the 'win98' directory to locate the desired files.
   
Last update: 2004.7.12
KEYTEC, INC.  Home of the Magic Touch
www.magictouch.com