
   Magic Touch USB-X & USB Controller Installation for Win98 & ME:

   1. If there is a previous installation of Magic Touch or other brand touch 
      screen driver on your computer, you must uninstall that driver first. 
   2. Insert the Magic Touch driver CD, the setup window appears.  (If the autorun 
      is disabled on your computer, the setup window will not open automatically, 
      and you need to click the START button and RUN setup from the CD.)
   3. Click to select the USB controller.
   4. Click install button.
   5. When prompted for restarting the computer, click OK and plug in the USB controller.
   6. After the Windows is restarted, double click and open the TouchUSB icon.  
      Click the calibration button to perform a 4-point calibration.
   7. Read user's manual for other functional options. 

Note: If installation wizard requests you to insert your 'Windows 98 cd,' you will need
to locate your Windows installation cd which should have come with your purchase of Windows
98.  Once located, point the wizard at the 'win98' directory to locate the desired files.   

Last update: 2004.7.12
KEYTEC, INC.  Home of the Magic Touch
www.magictouch.com