
   Magic Touch USB-X & USB Controller Installation for Win2000 & XP:

   1. If there is a previous installation of Magic Touch or other brand touch 
      screen driver on your computer, you must uninstall that driver first. 
   2. Insert the Magic Touch driver CD, the setup window appears.  (If the autorun 
      is disabled on your computer, the setup window will not open automatically, 
      and you need to click the START button and RUN setup from the CD.)
   3. Click to select the USB controller.
   4. Click install button.
   5. When prompted for plugin the USB controller, connect the controller to USB port 
      and click OK.
   6. When prompted for restarting the computer, click OK.
   7. After the Windows is restarted, double click and open the TouchUSB icon.  
      Click the calibration button to perform a 4-point calibration.
   8. Read user's manual for other functional options. 

Last update: 2004.7.12
KEYTEC, INC.  Home of the Magic Touch
www.magictouch.com