
   Magic Touch ProE-X & ProE Controller Installation for Win2000 & XP:

   1. If there is a previous installation of Magic Touch or other brand 
      touch screen driver on your computer, you must uninstall that driver first. 
   2. Insert the Magic Touch driver CD, the setup window appears.  (If the autorun 
      is disabled on your computer, the setup window will not open automatically, 
      and you need to click the START button and RUN setup from the CD.)
   3. Click to select the ProE controller.
   4. Click install button.
   5. When prompted for restarting the computer, plug in the ProE-X or ProE controller 
      and click OK.
   6. After the Windows is restarted,
      In Win 2K/XP: When hardware wizard shows, just click continue anyway.
   7. Double click and open the Touch232 icon.  Click the calibration button to perform 
      a 4-point calibration.
   8. Read user's manual for other functional options. 

   
Last update: 2004.7.12
KEYTEC, INC.  Home of the Magic Touch
www.magictouch.com